QC11K-6X3200

1. Main technical parameters

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| No. | Item | | Parameter | Unit | Remarks |
| 1 | Max cut-table thickness | | 6 | mm |  |
| 2 | Max cut-table width | | 3200 | mm |  |
| 3 | Tensile strength of steel  plate to be cut | | 450 | N/m m2 |  |
| 4 | Distance between upright columns | | 3600 | mm |  |
| 5 | Strokes | | 6-12 | n/min |  |
| 6 | Back gauge stroke | | 10-800 | mm |  |
| 7 | Cutting angle | | 0.5-2.5 | ° |  |
| 8 | Distance between  workbench and ground | | 700 | mm |  |
| 9 | Throat Depth | | 120 | mm |  |
| 10 | Length of the blade | | 3300 | mm |  |
| 11 | Internal Gear  Pump | Model | NB3-G25F/CP1-25-P-10R | | |
| 12 | Flow | 25 | L/min |  |
| 13 | Pressure | 31.5 | Mpa |  |
| 14 | Primary  Moto | Model | Y132M-4/(B35) | | |
| 15 | Rotation Rate | 1400 | r/min |  |
| 16 | Power | 7.5 | kw |  |
| 17 | Motor of  Backgauge | Model | YS-7134 | | |
| 18 | Rotation Rate | 1400 | r/min |  |
| 19 | Power | 0.55 | kw |  |
| 20 | Operating System | E21S | | | |
| 21 | Overall Dimensions | Length | 3700 | mm |  |
| Width | 1800 | mm |  |
| Height | 2000 | mm |  |